
Integrated Key Word Spotting and Image Classification Demo

# Introduction

This is a brief set of instructions to help set up the integrated Key Word Spotting and Image Classification demo on dual Cortex-M55 cores with Ethos-U55 NPU. A more detailed set of app notes is being written but this quick start guide is available for customers in the interim.

The demo consists of two applications: a Key Word Spotting (KWS) application runs on the Cortex-M55 High-Efficiency core (H55-HE / M55\_1) and at the same time an Image Classification application run on the Cortex-M55 High-Performance core (M55-HP / M55\_0).

When the demo is started, both cores are booted by the Secure Enclave. The KWS application on M55-HE uses continuously listens to the audio input from the built-in microphones on the Alif base board. When the word “Go” is recognized, a command is sent to the M55 HP core to initiate the image classification application. The image classification application uses the camera to detect objects and displays the image output of the camera to a display along with the results of the image classification in real time. The M55 HE continues to listen for keywords and upon detecting the word “Stop”, a command is sent to the M55 HP core to stop the image classification.




# Required Hardware and Setup

* Alif CPU board
* Alif Base board
* Camera module
* Display panel
* USB-to-UART (two)
* ULINKpro or ULINKpro D


## Connect Camera and Display

Make sure the development kit is not connected to a power source before proceeding.


Start with the camera module. Find the camera connector on the base board beside the coin cell battery holder and microSD slot. Lightly press the camera module’s ribbon cable connector into the base board connector. Not too much pressure is needed before you should feel a snap.



The display panel connects to J415. Start with lifting the black plastic latch to open the connector.



With the latch lifted place the display panel’s ribbon cable into the connector. Then press the latch down to lock the ribbon cable in place.



## Connect USB-to-UART Adapters

In the Getting Started with Bare Metal User Guide it shows how to connect your USB-to-UART adapter to SEUART as part of the board setup.

For this example, you will need two adapters. The first will be connected to UART2 and the second will be connected to UART4 for console output. Each UART is used by one of the M55 cores. Be sure to follow the precautions in the Getting Started Guide to make sure the 1.8V jumper is selected on the adapters.

Connect the first UART cable between your PC and UART2 on the base board:

* J413 pin 13 (UART2\_RX): Connects to TXDATA (blue wire or as noted above) on the cable
* J413 pin 14 (UART2\_TX): Connects to RXDATA (black wire or as noted above) on the cable
* J418 (any pin) (GND): Connects to GND (green wire or as noted above) on the cable

A picture containing text, electronics

Description automatically generated

Connect the second UART cable between your host PC and UART4 on the base board:

* J412 pin 11 (UART4\_RX): Connects to TXDATA (blue wire or as noted above) on the cable
* J412 pin 12 (UART4\_TX): Connects to RXDATA (black wire or as noted above) on the cable
* J417 (any pin) (GND): Connects to GND (green wire or as noted above) on the cable

A close-up of a circuit board

Description automatically generated with medium confidence

## Debug and Power

At this point you may make the final connections for debug and power.


* Connect the ULINKpro to the host PC and then the CPU board
* Connect the DevKit to a power source via microUSB cable

# Required Software and Setup

* Ubuntu 20.04 LTS or Ubuntu MATE 20.04 LTS ([link](http://cdimage.ubuntu.com/ubuntu-mate/releases/20.04/release/))
* Arm Development Studio ([link](https://developer.arm.com/downloads/-/arm-development-studio-downloads) – choose Linux 64-bit version)
* Arm Compiler for Embedded ([link](https://developer.arm.com/downloads/-/arm-compiler-for-embedded) – choose x86\_64 Linux version, not the AArch64)
* Oracle VirtualBox ([link](https://www.virtualbox.org/))

## Virtual Machine Setup

Follow the guide at this page to create an Ubuntu virtual machine using Virtual Box ([link](https://ubuntu.com/tutorials/how-to-run-ubuntu-desktop-on-a-virtual-machine-using-virtualbox)). You should proceed far enough to install the VirtualBox Guide Additions. This enables USB support and allows for using Arm DS to debug from within Ubuntu later in the guide. In the machine settings, under the USB category, add the ULINKpro to your USB Device filters. The ULINKpro is not available in Windows while the box is checked.



## Ubuntu Setup

With Ubuntu running, run the below commands to get the environment ready for development.

sudo apt update

sudo apt upgrade -y

# required dependencies for Arm Development Studio and Arm compiler

sudo apt install libncurses5 libc6-i386 lib32gcc1 lib32stdc++6 lib32z1


# required dependencies for ML Embedded Toolkit

sudo apt install curl dos2unix python-is-python3

snap install cmake –classic


## Arm Software Setup

Start with downloading the tgz file for Development Studio and then extract it.



Within the extracted folder is a shell script. Open a terminal window, navigate to the extracted folder, and run the shell script.

Next, download the tar.gz file for Arm Compiler and use sudo to extract it to /usr/local/bin/ArmClang



Add the ARM license server to your environment (if applicable)

sudo sh -c "echo export ARMLMD\_LICENSE\_FILE=PORT@IPADDRESS > /etc/profile.d/arm-license.sh"

After installing Arm Clang compiler we will need to add it to the path

sudo sh -c "echo export PATH=/usr/local/bin/ArmCompiler6.18/bin:$PATH > /etc/profile.d/arm-compiler.sh"

At the time of writing, the following software versions were used:

* Python 3.8.10
* Pip 22.1.2
* Arm Compiler 6.18
* cmake 3.23.2

# Building the Applications

The two applications are built separately. They can also be executed one at a time to demonstrate the individual application’s functionality. Later they are combined in a flash download for the Alif device so that it can be run on the device standalone, without requiring the debug environment.

## Building the Key Word Spotting for M55-HE

Private repository on Alif Semi GitHub account:

<https://github.com/alifsemi/ml-kws-ic-example-ensemble-share>

git clone https://github.com/alifsemi/ml-kws-ic-example-ensemble-share.git

cd ml-kws-ic-example-ensemble-share

git submodule init

git submodule update

python set\_up\_default\_resources.py --additional-ethos-u-config-name ethos-u55-128

The above python command will take some time, around a few minutes. If you get errors right at the beginning, try doing the following and run the command again:

sudo apt-get install python3-pip

sudo apt install python3-venv

Delete the folder resource-downloaded

Rerun the commands

After the python command completes, let’s continue the build process.

mkdir build

cd build

cmake -DTARGET\_PLATFORM=ensemble \

-DTARGET\_SUBSYSTEM=**RTSS-HE** \

-DCMAKE\_TOOLCHAIN\_FILE=scripts/cmake/toolchains/bare-metal-armclang.cmake \

-DUSE\_CASE\_BUILD=kws \

-Dkws\_MODEL\_TFLITE\_PATH=resources\_downloaded/kws/kws\_micronet\_m\_vela\_**H128**.tflite \

-Dkws\_FILE\_PATH=resources/kws/samples/down.wav \

-DCMAKE\_BUILD\_TYPE=Debug -DLOG\_LEVEL=LOG\_LEVEL\_DEBUG ..

make ethos-u-kws -j

The output should be in ml-kws-ic-example-ensemble-share/build/bin/ethos-u-kws.axf

## Building the Image Classification for M55-HP

Public repository <https://git:qhub.com/alifsemi/ensembleML/tree/image_demo>

git clone https://github.com/alifsemi/ensembleML.git

cd ensembleML

git checkout image\_demo

python download\_dependencies.py

If you get errors during download\_dependencies.py, delete the dependencies directory and try again. , try doing the following and run the command again:

mkdir build

cd build

cmake -DTARGET\_PLATFORM=ensemble \

-DTARGET\_SUBSYSTEM=RTSS-HP \

-DCMAKE\_TOOLCHAIN\_FILE=scripts/cmake/toolchains/bare-metal-armclang.cmake \

-DUSE\_CASE\_BUILD=img\_class \

-Dimg\_class\_MODEL\_TFLITE\_PATH=resources/img\_class/model/mobilenet\_softmax\_v2\_1.0\_224\_uint8\_vela\_H256.tflite \

-Dimg\_class\_FILE\_PATH=resources/img\_class/samples/cat.bmp \

-DCMAKE\_BUILD\_TYPE=Debug -DLOG\_LEVEL=LOG\_LEVEL\_DEBUG ..

make -j

The output should be in ensembleML/build/bin/ethos-u-img\_class.axf

# Running the Applications using Arm DS

How to run the applications using Arm Development Studio and the ULINKpro debug tool.

Open Arm Development Studio. Follow the steps from the Getting Started with Bare Metal Guide to “create a debug connection…” to the Alif Development Kit.

Graphical user interface, application

Description automatically generated

Follow the Getting Started Guide until you have a “.launch” file capable of connecting any core on the development kit.

## Running the M55-HE KWS Application

Create a copy of the “.launch” config called “ethos-u-kws.launch”.

Open the launch config and choose the Cortex-M55\_1 in the “Connection” tab.

Graphical user interface, text, application, chat or text message

Description automatically generated

Then use the ethos-u-kws.axf file built from the steps before in the “Files” tab.

Graphical user interface, text, application, chat or text message, email

Description automatically generated

Finally, select “Debug from symbol: main” and close.

You should be able to run the application and see the below in the very first lines of output from UART2

Text


Description automatically generated

The application will run in a loop listening to the microphones. It will report if the keywords from the following list are spotted: up, down, left, right, yes, no, go, stop, on, off

Correct behavior:



Detection of left and right key words



Incorrect behavior (mics not working):



## Running the M55-HP Image Classification Application

Create a copy of the “.launch” config called “ethos-u-img-class.launch”.

Open the launch config and choose the Cortex-M55\_0 in the “Connection” tab.

Graphical user interface, text, application, chat or text message

Description automatically generated

Then use the ethos-u-img-class.axf file built from the steps before in the “Files” tab.

Graphical user interface, text, application, chat or text message

Description automatically generated

Finally, select “Debug from symbol: main” and close.

You should be able to run the application and see the below in the very first lines of output from UART2

# Running the demo using binaries

Convert built binary to bin format and copy to your current SETOOLS app-release folder. Do this for both applications.

cd build

cd bin

fromelf -v --bin --output ethos-u-kws.bin ethos-u-kws.axf

Copy the binaries to the app release directory build/images

Note, if you see a warning, when writing the binaries to MRAM, about the binaries not being aligned then use one of the following commands to pad out the binaries.

truncate --size /16 build/images/image\_name.bin

python3 pad\_16bytes.py -b build/images/image\_name.bin

The next step is to generate the binary ATOC image for the two programs.  Create a new JSON file called <app-release>/build/config/kws\_img\_class\_demo.json with the following content.

{

"HP\_Image": {

"binary": "ethos-u-img\_class.bin",

"version" : "1.0.0",

"mramAddress": "0x80001000",

"cpu\_id": "M55\_HP",

"flags": ["boot"],

"signed": false

},

"HE\_Voice": {

"binary": "ethos-u-kws.bin",

"version" : "1.0.0",

"loadAddress": "0x62000000",

"cpu\_id": "M55\_HE",

"flags": ["boot", "load"],

"signed": false

}

}

Next, run app-gen-toc.py to generate the package image, which will be written to the file AppTocPackage.bin in the build directory. We will use the “-f” option to specify the input filename (kws\_img\_class\_demo.json) for the configuration file we just created. Execute this command:

python app-gen-toc.py --filename build/config/kws\_img\_class\_demo.json

Write the applications using the SETOOLS command

python app-write-mram.py

Outputs to the UART2 (kws) and UART4 (image classification)